품 명		스테레오 액티브 DI 박스
모 델		DI2	제조사	LA AUDIO
Technical Specifications
	ELECTRICAL Frequency response : 20Hz-20kHz (+0 -2dB) Signal to Noise ratio : > 100dB (0dB gain), > 85dB (+20dB gain) Input impedance : Normal: 1M, Pad: 10k Output impedance : 330R (Balanced), 2k2k (Unbalanced) Load impedance : > 300R (Balanced), > 2k (Unbalanced) THD : < 0.025% (0dB Gain), < 0.12% (+20dB Gain) Phantom Power : 15-48 volts Phantom supply : 1mA (1k2 load) Batteries : 2 x 9V batteries PP3, 1604 PHYSICAL Connectors : Input: 1/4" jack, Link: 1/4" jack Unbalanced Output : 1/4" jack Balanced output : Male XLR 3 pin (Pin 2 hot) Dimensions (mm) : 105 (4.75") W, 50 (3.75") H, 125 (2.25") D Weight : 0.3kg Shipping weight : 0.36kg Operating temperature : 0°C to +50°C Storage temperature : -30°C to +75°C

(주)사운드솔루션

3) 스테레오 액티브 DI 박스

1. 개  요

DI2 Mk3는 한 개의 채널을 사용할 수 있는 고급형 액티브 타입의 DI 박스로서 반영구적인 알루미늄 케이스로 구성되어 있습니다. 팬텀 전원을 사용할 수 있으며, 내부에 두 개의 PP3 밧데리를 내장할 수도 있습니다. 아주 낮은 소비전력을 가진 회로를 사용하기 때문에 밧데리를 사용하여 300 시간 이상 사용이 가능합니다.

실수로 인한 밧데리 방전을 미연에 차단하기 위하여 팬텀 파워를 자동으로 감지하는 기능을 가지고 있는 것은 물론 입력 신호가 연결되지 않은 상태에서는 자동으로 전원이 꺼집니다.

DI2 Mk3는 다용도로 사용할 수 있는 링크 입력, 발란스 및 언발란스 출력, 입력 및 출력 레벨 조정 스위치 및 그라운드 리프트 스위치를 제공합니다. 전원 상태를 확인할 수 있는 LED를 제공함으로써 보다 사용의 편의성을 더하였습니다.

DI2는 액티브 타입의 회로를 사용하기 때문에 시그널에 대한 보다 뛰어난 명료도를 얻을 수 있으며, 발란스 출력을 통해 아주 먼 거리까지 안정적인 신호를 보낼 수 있어, 신호에 대한 손실 없이 아주 큰 규모의 공연장에서 보다 효율적으로 사용할 수 있습니다.

2. 기능 및 특성

액티브 타입 디자인

1 MΩ의 입력 임피던스 및 +10 dBm의 라인 레벨 출력

300 W 스피커 입력 가능

반 영구적인 알루미늄 재질의 케이스

자동 전원 꺼짐 회로

1/4” TRS 출력을 사용하여 아주 먼 거리까지 안정적인 발란스 신호 전송 가능

낮은 레벨의 픽업에서 사용할 수 있도록 20 dB 게인 스위치 제공

내부 밧데리 및 외부 팬텀 파워를 자동으로 감지하여 적용하는 오토 스위칭 기능

3. 사  양

ELECTRICAL

Frequency response : 20Hz-20kHz (+0 -2dB)

Signal to Noise ratio : > 100dB (0dB gain), > 85dB (+20dB gain)

Input impedance : Normal: 1M, Pad: 10k

Output impedance : 330R (Balanced), 2k2k (Unbalanced)

Load impedance : > 300R (Balanced), > 2k (Unbalanced)

THD : < 0.025% (0dB Gain), < 0.12% (+20dB Gain)

Phantom Power : 15-48 volts

Phantom supply : 1mA (1k2 load)

Batteries : 2 x 9V batteries PP3, 1604

PHYSICAL

Connectors : Input: 1/4" jack, Link: 1/4" jack

Unbalanced Output : 1/4" jack

Balanced output : Male XLR 3 pin (Pin 2 hot)

Dimensions (mm) : 105 (4.75") W, 50 (3.75") H, 125 (2.25") D

Weight : 0.3kg

Shipping weight : 0.36kg

Operating temperature : 0°C to +50°C

Storage temperature : -30°C to +75°C

*  DI 2 동등이상품.