WIRELESS GUITAR PEDAL TUNER & RECEIVER

1) 기    능

본 기기는 풋 컨트롤을 위한 기타 페달 튜너 겸 수신기로서 2.4㎓ 주파수 내 최대 8채널 동시 사용이 가능하여야 한다. 자동 주파수 관리 기능이 있어 최적의 채널을 검색할 수 있고 송신기의 게인 컨트롤을 원격으로 조정할 수 있어야 한다.

2) 기기특성

- Tuning Bandwidth	: 2400~2483.5 MHz

- Working Range	: 60 m (200 ft) typical

(Note : Actual range depends on RF signal absorption, reflection and interference.)

- Transmit Mode	: Frequency Hopping

- Audio Frequency Response	: 20 Hz ~ 20 kHz

(Note : Dependent on microphone type)

- Dynamic Range	: 120 dB, A-weighted

- RF Sensitivity	: -88 dBm, typical

- Total Harmonic Distortion	: 0.2%, typical

- RF Output Power	: 10 mW E.I.R.P. max

- Operating Temperature Range	: -18°C (0°F) to 57°C (135°F)

(Note : Battery characteristics may limit this range.)

- Storage Temperature Range	: -29°C (-20°F) to 74°C (165°F)

- Polarity	: Positive pressure on microphone diaphragm (or positive voltage applied to tip of WA302 phone plug) produces positive voltage on pin 2 (with respect to pin 3 of low-impedance output) and the tip of the high impedance 1/4-inch output.

- Battery Life	: Up to 16 hours

- Power Requirements	: 9 to 15 V DC @ 550 mA, supplied by external power supply

* GLXD6 또는 동등 이상의 제품이어야 한다.